**SECTION 28 23 19**

**DIGITAL VIDEO RECORDERS AND ANALOG RECORDING DEVICES**

**Uniview Technology HNRX04 Hybrid Network Recorder**

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

*This guide specification is intended for use by the design/construction professional and any user of Uniview Technology products to assist in developing project specifications for security and video surveillance systems.*

*Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

1. **GENERAL**
	1. SUMMARY
		1. Section includes Digital Video Recorders and Analog Recording Devices.
		2. Related Sections:
			1. Section 28 23 13 – Video Surveillance Control and Management Systems
			2. Section 28 23 16 – Video Surveillance Monitoring and Supervisory Interfaces
			3. Section 28 23 26 – Video Surveillance Remote Positioning Equipment
			4. Section 28 23 23 – Video Surveillance Systems Infrastructure
	2. SYSTEM DESCRIPTION
		1. Description: Video surveillance and monitoring at points as indicated on Drawings.
			1. HNRX04: 4ch Analog / 2ch IP, 8MP Resolution, Hybrid Network Recorder
		2. Performance Requirements
			1. Fully integrated, stand-alone video recording solution for network surveillance systems of up to 6 channels (cameras).
			2. Capable of recording 3840 x 2160, 8MP resolution video images with H.264 compression
			3. ONVIF compliant for network video interoperability
			4. Connect and record up to four (4) analog camera and two (2) network IP cameras
			5. 1920 x 1080 display capability on HDMI monitor output.
			6. Concurrent displays on HDMI and VGA monitor outputs.
			7. 2-way audio communication
			8. Stable embedded operating system.
			9. Easy plug and play functionality with automatic device discovery and display
			10. Maximum incoming throughput of 48Mbps and Outgoing of 60Mbps
			11. Maximum 1 SATA HDD up to 10TB each
			12. Supports Mobile Phone Applications with Apple and Android Operating Systems
			13. Pan-Tilt-Zoom (PTZ) camera control
			14. Long range transmission distance over RG-6 coax cable up to 2000ft (600m)
	3. DEFINITIONS
		1. H.265 (also known as MPEG-H Part 2): a powerful encoding format that has become the successor to H.264 (MPEG-4 Part 10) standard. Recording video in H.265 format requires approximately 50% less storage than video recorded with H.264.
		2. PTZ: refers to a movable camera that has the ability to pan left and right, tilt up and down, and zoom or magnify a scene.
	4. SUBMITTALS
		1. Submit under provisions of Section 01 33 00 - Submittal procedures.
		2. Shop Drawings: Indicate electrical characteristics and connection requirements, including system wiring diagram.
		3. Product Data: Submit catalog data showing electrical characteristics and connection requirements for each component.
	5. CLOSEOUT SUBMITTALS
		1. Section 01 70 00 - Execution and Closeout Requirements: Closeout procedures.
		2. Project Record Documents: Record actual locations of cameras and routing of cabling.
		3. Operation and Maintenance Data: Submit instructions for operating system and performing routine trouble shooting procedures.
	6. QUALIFICATIONS
		1. Manufacturer: Company specializing in manufacturing products specified in this section with minimum ten years documented experience.
		2. Supplier: Authorized distributor of specified manufacturer with minimum 5 years documented experience.
		3. Installer: Authorized installer of specified manufacturer with 5 years documented experience and with service
	7. ENVIRONMENTAL REQUIREMENTS
		1. Section 01 60 00 - Product Requirements.
		2. Deliver materials in manufacturer’s original, unopened, undamaged packaging; and unharmed original identification labels.
		3. Protect store materials from environmental and temperature conditions following manufacturer’s instructions.
		4. Handle and operate products and systems according to manufacturer’s instructions for installation, environmental, mechanical or electrical requirements and within thermal stress limits.
		5. Ensure conformance with operating limitations according to applicable data sheet.
	8. FIELD MEASUREMENTS
		1. Verify field measurements prior to fabrication.
	9. WARRANTY
		1. Provide manufacturer’s warranty covering [3] years for CCTV products to repair or replace defective equipment.
		2. Exchanges available for product failures.
	10. MAINTENANCE SERVICE
		1. Section 01 70 00 - Execution and Closeout Requirements: Maintenance service.
		2. Make ordering of new equipment for expansions, replacements, and spare parts available to dealers and end users.
		3. Provide factory direct technical support via phone or e-mail, or any time via Web.
			1. Provide toll-free numbers to contact customer support.
		4. Provide on-site training and on-line training via web.
2. PRODUCTS
	1. DIGITAL VIDEO RECORDERS
		1. Manufacturers:
			1. Uniview Technology
			2. Substitutions: Section 01 60 00 - Product Requirements: Not Permitted.
		2. Model: HNRX04
		3. Product Description: 4ch Analog / 2ch IP, 8MP Resolution, Hybrid Network Recorder
		4. General Requirements:
			1. The HNRX04 Network Recorder (NVR) shall provide these features:
				1. Flexible and scalable network video management system in an easy to use versatile design.
				2. View, record, and control cameras, handle alarms and check device status through one interface.
				3. Simultaneously view and record video from up to 6 different analog and IP video sources
				4. 100M network interface
				5. Remote configuration and management of devices on surveillance system.
				6. Easy Plug and Play functionality with automatic device discovery and display
				7. Internal storage of one (1) SATA HDD, up to 10TB.
				8. Capable of delivering live video to mobile devices
		5. The HNRX04 shall support up to 4 analog video inputs with adaptive access on multiple formats:
			1. AHD
			2. TVI
			3. CVI
			4. CVBS (960H)
		6. The HNRX04 shall support up to 2 network IP video inputs (or up to 6 inputs if analog cameras are not connected)
		7. The HNRX04 NVR shall feature H.265 video compression to reduce bandwidth and storage requirements.
		8. The HNRX04 NVR shall be capable of recording up to 3840 x 2160 resolution video images.
		9. The HNRX04 NVR shall provide 3rd party network IP camera connectivity for ONVIF compatible cameras.
		10. The HNRX04 NVR shall be capable of displaying Full HD, 1920 x 1080 output on a HDMI and VGA monitors
		11. The HNRX04 NVR shall provide Network Time Synchronization and Daylight Savings Time change functionality.
		12. The HNRX04 NVR shall offer email notifications generated by programmed alarm activity
		13. The HNRX04 NVR shall support mobile phone applications for iPhone and Android.
		14. The HNRX04 NVR shall have multiple simultaneous functions with single software interface:
			1. Live viewing
			2. Recording
			3. Playback
			4. Network transmission
			5. Backup (Export)
		15. The HNRX04 shall have long range transmission distance over RG-6 coax cable up to 2000ft (600m)
		16. Electrical:
			1. Input Power: 12VDC
			2. Power Consumption: 8W (w/o HDD)
		17. Video
			1. Analog camera inputs: 4 x BNC
			2. IP camera inputs: 1 x RJ45 Ethernet connector
			3. Supported analog video format: AHD, TVI, CVI, CVBS (960H)
			4. Supported network IP video format: H.265
			5. Supported video resolution: up to 3840 x 2160
			6. Maximum Playback Frame Rate (fps):
				1. Analog & IP Cameras: 4 x 4MP @30
				2. IP Cameras Only: 4 x 4MP @30
		18. Storage:
			1. Internal HDD: SATA, 1 bay, 10TB maximum
			2. Backup: USB 2.0
		19. Network
			1. Supported Protocols: TCP/IP, P2P, UPnP, NTP, DHCP, PPPoE
			2. Remote Access: Guard Station Client Software; Web Browser; Mobile Apps for iPhone and Android Devices
			3. Web Browsers: IE, Firefox, Chrome, Opera
			4. Remote Connections: 128 Users
			5. Bandwidth Throughput (Maximum): 48Mbps Incoming, 60Mbps outgoing
		20. General
			1. Analog Connector: BNC
			2. Ethernet: 1 x RJ45 Port; 10Mbps / 100Mbps
			3. USB: 2 x USB2.0, rear panel
			4. RS-485 Serial Port: Terminal block
			5. Audio
				1. Input: 1 RCA
				2. Output: 1 RCA
			6. Operating Temperature: -10°C ~ +55°C (+14°F ~ +131°F)
			7. Humidity: 0%RH ~ 90%RH
			8. Dimensions (W x D x H): 260 × 240 × 44mm (10.2 × 9.4 × 1.7")
			9. Weight: 2.473bs (1.1kg) (w/o HDD)
		21. Conformity Certifications:
			1. Federal Communications Commission (FCC)
			2. European Conformity (CE)
			3. Underwriters Laboratories (UL) (Power Supply Only)
		22. Accessories
			1. Multi-Function Video Test Monitor: 4KTESTMON
			2. 8-port PoE Switch: NSW081P
3. EXECUTION
	1. EXISTING WORK
		1. Disconnect and remove abandoned video surveillance equipment.
		2. Extend existing video surveillance installations using materials and methods compatible with existing installations as specified.
		3. Clean and repair existing video surveillance equipment remaining or to be reinstalled.
	2. EXAMINATION
		1. Examine areas to receive devices and notify adverse conditions affecting installation or subsequent operation.
		2. Do not begin installation until unacceptable conditions are corrected.
		3. Non-compliance with security instructions may result in loss of data.
		4. Ensure environmental, mechanical and electrical requirements are met.
	3. PREPARATION
		1. Protect devices from damage during construction.
	4. INSTALLATION
		1. Install devices in accordance with manufacturer’s instruction at locations indicated on the floor plan drawings.
		2. Perform installation with qualified service personnel.
		3. Install devices in accordance with the National Electrical Code or applicable local codes.
		4. Ensure selected location is secure and offers protection from accidental damage.
			1. Ground and bond video surveillance equipment in accordance with Section 26 05 26.
		5. Location must provide reasonable temperature and humidity conditions, free from sources of electrical and electromagnetic interference.
	5. FIELD QUALITY CONTROL
		1. Test proper operation of all video system devices.
			1. Communication between recorder and cameras.
			2. Independent operation of alarms, and cameras.
		2. Test proper operation of software programs.
		3. Determine and report all problems to the manufacturer’s customer service department.
	6. MANUFACTURER'S FIELD SERVICES
		1. Section 01 40 00 - Quality Requirements: Manufacturer's field services.
		2. Furnish manufacturer’s field representative to supervise final wiring connections and system adjustments.
	7. ADJUSTING
		1. Section 01 70 00 - Execution and Closeout Requirements: Requirements for starting and adjusting.
		2. Make proper adjustment to video system devices for correct operation in accordance with manufacturer’s instructions.
		3. Make any adjustment of camera settings to comply with specific customer’s need.
	8. DEMONSTRATION AND TRAINING
		1. Demonstrate at final inspection that video management system and devices function properly.

END OF SECTION